================================================================================
                                样例使用说明
                                Sample Description
================================================================================
功能描述：
此样例演示了SCI的中断方式发送和接收不定长数据，SCI配置为115200，数据位8，停止位1，
校验位None,下载并运行程序后，然后通过上位机下发任意长度个数据（不超过128bytes），
例如0x1~0xC,则MCU会把接收到的数据再次发送到上位机。

Function descriptions:
This example demonstrates the interrupt method of SCI to send and receive
variable length data. SCI is configured as 115200, with data bit 8, stop bit
1, and check bit None. After downloading and running the program, the MCU will
send any length of data (not exceeding 128bytes) through the upper computer,
such as 0x1~0xC. The MCU will send the received data to the upper computer again.
================================================================================
测试环境：
测试用板：PY32CA80_STK
MDK版本： 5.28

Test environment:
Test board: PY32CA80_STK
MDK Version: 5.28
================================================================================
使用步骤：
1. 编译并下载程序到MCU，并运行；
2. 通过USB转TTL模块连接PC与STK板,STK板与USB转TTL模块的连线方式如下；
STK板         USB转TTL模块
PC6(TX)  -->  RX
PC5(RX)  -->  TX
GND      -->  GND
3. PC端打开串口调试助手，正确连接上通讯COM口；
4. 上位机发送任意长度个数据（不超过128bytes），MCU会将接收到的数据回发给上位机

Example execution steps:
1. Compile and download the program to MCU and run it;
2. Connect the PC to the STK board through the USB to TTL module, and the connection
method between the STK board and the USB to TTL module is as follows:
STK board     USB to TTL module
PC6(TX)  -->  RX
PC5(RX)  -->  TX
GND      -->  GND
3. Start the serial assistant on the PC, correctly connect the COM port.
4. The upper computer sends any length of data (not exceeding 128 bytes), and
the MCU will send the received data back to the upper computer
================================================================================
注意事项：

Notes:

================================================================================