================================================================================
                                样例使用说明
                                Sample Description
================================================================================
功能描述：
此样例演示了TIM1的单脉冲模式。配置TIM1为从模式触发模式，触发源为TI2FP2，通道1为
PWM2模式，映射到PB7，通道2为输入模式，映射到PB0。当PB0上检测到一个上升沿时，PB7
延迟20ms后产生一个宽度为80ms的脉冲。

Function descriptions:
This sample demonstrates the single pulse mode of TIM1. TIM1 is configured in 
slave mode trigger mode with TI2FP2 as the trigger source. Channel 1 is 
configured as PWM mode 2 and mapped to pin PB7, while channel 2 is configured 
as input mode and mapped to pin PB0. When an rising edge is detected on PB0, 
a 20ms delay is applied, and then PB7 will output a pulse with a width of 80ms.
================================================================================
测试环境：
测试用板：MS32C001B_STK
MDK版本： 5.28
IAR版本： 9.20
GCC 版本：GNU Arm Embedded Toolchain 10.3-2021.10

Test environment:
Test board: MS32C001B_STK
MDK Version: 5.28
IAR Version: 9.20
GCC Version: GNU Arm Embedded Toolchain 10.3-2021.10
================================================================================
使用步骤：
1. 编译下载程序到MCU，并运行；
2. 使用示波器的捕获模式观察PB7，PB0；
3. 当PB0上产生一个上升沿时，延迟20ms后PB7输出一个宽度为80ms的脉冲。

Example execution steps:
1.Compile and download the program to the MCU, and then run it.
2.Use an oscilloscope in capture mode to observe pins PB7 and PB0.
3.When a rising edge is detected on PB0, after a delay of 20ms, PB7 will 
output a pulse with a width of 80ms.
================================================================================
注意事项：

Notes:

================================================================================